**Concealment Warranty**

**Ehresmann Branch Installation Guide and Warranty**

1. Ehresmann branches will be under a (3) three year warranty with contingency of up to 4 or 5 years from date of shipment- provided they are properly handled and installed. This warranty includes branch replacement only and does not include freight or installation expenses.
2. All branch materials including slip pipes, top cap and hardware must be inventoried upon receipt. Any missing or damaged parts (in transit to site) will be replaced if notified below. **Any damaged branches identified after truck off-load will be the responsibility of the installation crew.**
3. Our branches must be installed per our specific installation procedure or this warranty will be null & void.
4. EEI HDPE pine branches should be handled with care during off-load, installation, and/or storage. **Branch assemblies are to be handled from the *pipe end only.***
5. Once installed, the branches should not to be used in lieu of a tower climb system.
6. If the branches are thrown, dropped or mishandled they can crack or break.
7. Cracked branches should not be installed.
8. **Branch crates should be lifted from the sides with a minimum fork length of 6’-0”.**
9. **We cannot over iterate the importance of proper handling during transportation, offload, any storage and installation of Ehresmann branches.**

***All branches have been received in good condition and I assume full responsibility of their care during the installation. I acknowledge I have read and fully understand this branch installation guide and agree to these instructions.***

Crew Foreman: ***\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*** *(signature required)*

Site Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date materials received:\_\_\_\_\_\_\_\_\_\_\_\_

Please indicate any damaged or missing items below:

1. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
2. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
3. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

This sheet can be faxed to: Ehresmann Engineering @ (605) 665-9780

***\*\*An Ehresmann representative will be available to oversee any branch installation on site if requested at additional expense****. 10/10/2016*